Hey, this is Eduardo. This GUI generates a generic TTL pulse waveform (5V) using the ni-USB 6215.

We used to Trigger the DS8R electrical stimulator.

You need to install: PyDAQmx, PyQt5.